# Debugger

Note, if you are looking for a graphical front-end for the bochs debugger, you may want to check out BFE. This is a package written by a bochs user which can interface with the text based bochs debugger. No linking is necessary. It's not part of bochs, but you may find it useful.

You can now conditionally compile in a GDB like command line debugger, that allows you to set breakpoints, step through instructions, and other useful functions. If there isn't a command for something you believe is generally useful for the debugger, let me know and I'll implement it if possible.

To use the debugger, you must configure bochs with the '--enable-debugger' and '--enable-disasm' flags. For example:

      ./configure --enable-debugger --enable-disasm

NOTE: You must use flex version 2.5.4 or greater. I have heard that version 2.5.2 will not work.

When you first start up bochs, you will see the command line prompt

      bochs:1>

From here, you may use the following commands:

### Execution Control

      c                           Continue executing
      stepi [count]               execute count instructions, default is 1
      si    [count]               execute count instructions, default is 1
      step  [count]               execute count instructions, default is 1
      s     [count]               execute count instructions, default is 1
      Ctrl-C                      stop execution, and return to command line prompt
      Ctrl-D                      if at empty line on command line, exit
      quit                        quit debugger and execution
      q                           quit debugger and execution

### BreakPoints

      NOTE: The format of 'seg', 'off', and 'addr' in these descriptions,
            are as follows.  I don't have any way to set the current radix.

            hexidecimal:    0xcdef0123
            decimal:        123456789
            octal:          01234567

      vbreak seg:off              Set a virtual address instruction breakpoint
      vb     seg:off

      lbreak addr                 Set a linear address instruction breakpoint
      lb     addr

      pbreak [*] addr             Set a physical address instruction breakpoint
      pb     [*] addr             (the '*' is optional for GDB compatibility)
      break  [*] addr
      b      [*] addr

      info break                  Display state of all current breakpoints
      delete n                    Delete a breakpoint
      del    n
      d      n

### Manipulating Memory

      x  /nuf addr      Examine memory at linear address addr
      xp /nuf addr      Examine memory at physical address addr
         n              Count of how many units to display
         u              Unit size; one of
                          b Individual bytes
                          h Halfwords (2 bytes)
                          w Words (4 bytes)
                          g Giant words (8 bytes)
                          NOTE: these are *not* typical Intel nomenclature sizes,
                                but they are consistent with GDB convention.
         f              Printing format.  one of
                          x Print in hexadecimal
                          d Print in decimal
                          u Print in unsigned decimal
                          o Print in octal
                          t Print in binary

        n, f, and u are optional parameters.  u and f default to the last values
        you used, or to w(words) and x(hex) if none have been supplied.
        n currently defaults to 1.  If none of these optional parameters are
        used, no slash should be typed.  addr is also optional.  If you don't
        specify it, it will be the value the next address (as if you had
        specified n+1 in the last x command).

      setpmem addr datasize val    Set physical memory location of size
                                   datasize to value val.

      crc  addr1  addr2            Show CRC for physical memory range addr1..addr2
      info dirty                   Show physical pages dirtied (written to) since last display
                                   Values displayed are the top 20 bits only (page addresses)

### Info

      info program      Execution status of the program
      info registers    List of CPU integer registers and their contents
      info break        Information about current breakpoint status

### Manipulating CPU Registers

      set $reg = val    Change a CPU register to value val.  Registers may be one of:
                          eax, ecx, edx, ebx, esp, ebp, esi, edi.
                        Currently, you may not change:
                          eflags, cs, ss, ds, es, fs, gs.

        Examples: set $eax = 0x01234567
                  set $edx = 25

      info registers    See Info section
      dump_cpu          Dump complete CPU state
      set_cpu           Set  complete CPU state

        Format of "dump_cpu" and "set_cpu":
        "eax:0x%x\n"
        "ebx:0x%x\n"
        "ecx:0x%x\n"
        "edx:0x%x\n"
        "ebp:0x%x\n"
        "esi:0x%x\n"
        "edi:0x%x\n"
        "esp:0x%x\n"
        "eflags:0x%x\n"
        "eip:0x%x\n"
        "cs:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "ss:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "ds:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "es:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "fs:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "gs:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "ldtr:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "tr:s=0x%x, dl=0x%x, dh=0x%x, valid=%u\n"
        "gdtr:base=0x%x, limit=0x%x\n"
        "idtr:base=0x%x, limit=0x%x\n"
        "dr0:0x%x\n"
        "dr1:0x%x\n"
        "dr2:0x%x\n"
        "dr3:0x%x\n"
        "dr4:0x%x\n"
        "dr5:0x%x\n"
        "dr6:0x%x\n"
        "dr7:0x%x\n"
        "tr3:0x%x\n"
        "tr4:0x%x\n"
        "tr5:0x%x\n"
        "tr6:0x%x\n"
        "tr7:0x%x\n"
        "cr0:0x%x\n"
        "cr1:0x%x\n"
        "cr2:0x%x\n"
        "cr3:0x%x\n"
        "cr4:0x%x\n"
        "inhibit_int:%u\n"
        "done\n"

        Notes:
          - s is the selector
          - dl is the shadow descriptor low  dword (4 byte quantitiy)
          - dh is the shadow descriptor high dword (4 byte quantitiy)
          - valid denotes if the segment register holds a validated shadow descriptor
          - inhibit_int is set if the previous instruction was one which delays the
              acceptance of interrupts by one instruction (STI, MOV SS)
          - any errors encountered by the set_cpu command, are reported by
            "Error: ...".  They may be reported after any of the input lines,
            or after the "done" line, during limit checks.
          - A successful set_cpu command ends with the separate line:
            "OK".

### Disassembly commands

      disassemble start end       Disassemble instructions in given linear address
                                  range, inclusive of start, exclusive of end.
                                  Use "set $disassemble_size =" to tell
                                  debugger desired segment size.  Use a value for
                                  end of less than start (or zero) if you only
                                  want the first instruction disassembled.
      set $disassemble_size = n   Tell debugger what segment size to use when
                                  the "disassemble" command is used.  Use values
                                  of 16 or 32 for n.  Default is 32.

      set $auto_disassemble = n   Cause debugger to disassemble current instruction
                                  every time execution stops if n=1.  Default is 0.
                                  Segment size of current CPU context is used for
                                  disassembly, so variable "$disassemble_size" is
                                  ignored.

### Instrumentation

    To use instrumentation features in bochs, you must compile in support for it.
    You should build a custom instrumentation library in a separate directory in
    the "instrument/" directory.  To tell configure which instrumentation library
    you want to use, use the "--enable-instrumentation" option.

    The default library consists of a set of stubs, and the following are
    equivalent:

      ./configure [...] --enable-instrumentation
      ./configure [...] --enable-instrumentation="instrument/stubs"

    You could make a separate directory with your custom library,
    for example "instrument/myinstrument", copy the contents of
    the "instrument/stubs" directory to it, then customize it.  Use:

      ./configure [...] --enable-instrumentation="instrument/myinstrument"

### Instrumentation commands

      instrument start            calls bx_instr_start()
      instrument stop             calls bx_instr_stop()
      instrument reset            calls bx_instr_reset()
      instrument print            calls bx_instr_print()

## New Commands

### trace-on

Disassemble every executed instruction. Note that instructions that cause exceptions are not really executed, and therefore not traced.

### trace-off

Disable tracing.

### ptime

Print the current time (number of ticks since start of simulation (modulo 2^32)).

### sb delta

Insert a time break point delta instructions into the future.

### sba time

Insert a time break point at time.

### record filename

Record console input to file filename. The file consists of zero or more lines of the form "%s %d %x", where the first word is the event type, the second is a time stamp and the third is event specific data.

### playback filename

Playback console input from file filename. Additional input can be given directly in the console window. Events in the file will be played back at times relative to the time when the playback command was executed.

### print-stack [num words]

Print the num words top 16-bit words on the stack. Num words defaults to 16. Only works reliably in protected mode when the base address of the stack segment is zero.

### watch stop

Stop the simulation (and return to prompt) when a watch point is encountered.

### watch continue

Do not stop the simulation when watch points are encountered. They will still be logged.

### watch

Print current watch point status.

### unwatch

Remove all watch points.

### watch read address

Insert a read watch point at physical address address.

### watch write address

Insert a write watch point at physical address address.

### unwatch read address

Remove read watch point from physical address address.

### unwatch write address

Remove write watch point from physical address address.

### modebp [string]

Insert documentation here.

### load-symbols [global] filename [offset]

Load symbols from file filename. If the global keyword is added, then the the symbols will be visible in all contexts for which symbols have not been loaded. Offset (default is 0) is added to every symbol entry. The symbols are loaded in the current (executing) context.

The symbol file consists of zero or more lines of the format `"%x %s"`.

### show [string]

Insert documentation here.

## Resource file extensions

### time0: time

Specifies the start (boot) time of the virtual machine. Use a time value as returned by the time(2) system call. Time equal to 1 is a special case which starts the virtual machine at the current time of the simulator host.

### cdromd: dev=device, status=(inserted|ejected)

LoseNT needs a CD in order to boot properly. Our simulated CD-ROM unit communicates directly with the CD-ROM driver in Linux. Device is a device special file to which the CD-ROM driver is connected (typically /dev/hdc). Device is ignored if status=ejected.

Related Links:

- Cosimulation
- Instrumentation