0.0.4 :
	Updated busybox
	New logo
0.0.3 :
	New features :
		- reboot
		- shutdown




How to use ED@chip


First, Upgrade your SmartXX to at least revision 3245.
(you can upgrade with your webbrowser too ! , no need to flash over CD or HDD)
Simple flash to ANY bank you find in the Flash Menu (+ follow instructions them)

You find the upgrade on SmartXX downloadsite.

Then, go to BankMenu
-> Config
-> Bios / Bank Config
-> Bankmode (Mid 2MB) 	/ You have to hold both triggers while moving there
-> Select 2048	(press A)

-> Flash ed_on_chip then into the 2MB bank (displayed) !

The IP you had in SmartXX OS, will be used in ED@chip II

Ed @ chip takes some seconds to boot, so don't worry

after it has bootet, you can FTP into your xbox.
the
User: xbox 
PW:   xbox


Telnet works, too :-)


by SmartXX Team.





