TEAM JUSTMODIT

JUSTMODIT.COM


Here are the instructions for cloning a Hard Drive for your XboX system. Please read all the instructions before you begin!

1. You will need two identical (Manufacture and Size) Hard Drives the first (Master)(hda) will have all the data you want to copy. The second (Slave)(hdb) will be the blank. *Note* BE SURE WHEN YOU REMOVE THE HARD DRIVE FROM YOUR XBOX YOU MARK IT AS THE MASTER YOU DO NOT WANT TO GET THE DRIVES MIXED UP!!!

2. You will need a blank floppy disk. Insert the blank floppy into your drive and run the program winrawrite.exe (found inside the zip file). Open the file called trinux-0.80rc2-ide.img (also found inside the zip file) then click Write. This will create your bootable Linux disk.

3. After you have completed the above steps you need to shut your computer down.

4. You will need to disconnect all of the IDE Devices in your computer and use the cable on IDE1 on the motherboard to connect the drives to. Set the jumpers on the HD with the data on it to the master settings and the jumpers on the empty drive to the slave setting. *Note* The master hard drive goes on the end position in the ribbon.

5. Next you will need to restart you computer with the bootable floppy disk in and the hard drives connected. Linux will start from the floppy. When it is done with the startup process you will get a # at the # you will type dd if=/dev/hda of=/dev/hdb then hit the enter key.

The cloning process will take up to 3-5 hours depending on drive size and weather you are using a 40 pin ide ribbon or an 80 pin the 80 pin ribbon is faster.


Team JustModIt
www.justmodit.com

PLEASE TAKE NOTE THAT WHEN YOU FIRST RUN THE PROGRAM IT MIGHT TAKE TIME TO LOAD, WHEN IT STARTS TO COPY IT WILL KEEP FLASHING LET IT COMPLETE THE CLONE TILL IT COMES TO A COMMAND PROMT (#) IT WILL TAKE A FEW HOURS TO COMPLETE